**Fluidized Bed Reactor**

**Equipment:** Fluidized bed reactor

**No. of Equipment: UJEP2**

**Responsible coordinator:** Mgr. Jindrich Matousek, Ph.D.

**Name of Institution: J**. E. Purkyně University in Ústí nad Labem, Faculty of Science, Department of Physics

**Address of Institution:** České mládeže 8, 400 96, Ústí nad Labem Czech Republic

**E-mail:** [j](mailto:petr.sazama@jh-inst.cas.cz)indrich.matousek@ujep.cz

**Telephone:** +420 475283 145

**Homepage:** http://www.sci.ujep.cz/

**Contact person:** Mgr. Jindrich Matousek, Ph.D.

**E-mail:** [j](mailto:petr.sazama@jh-inst.cas.cz)indrich.matousek@ujep.cz

**Telephone: +42**0 475283 145

**Equipment Description**

**Description of equipment:**

Equipment for plasma treatment of powder materials

Analytical equipment for surface analysis. - Secondary

Specifications and technical features:

Lower amounts of powder treatable (it is research reactor) – at the moment hundreds of mg to units g. The reactor is being developed to increase the capacity.

Working gases: Ar, O2, H2, N2, …

Working gas pressure: hundreds of Pa

RF Power: up to 200W

**Specification of expertise relevant to NanoEnviCz workpackages:**

**WP3**a,g, **WP4**a,c, **WP5**a, **WP6**a-e, **WP7**a,d,

**Detailed description of expertise**

**Please, specify the main research topics connected with equipment**:

Plasma treatment of powder materials

Any material in powder form can be plasma treated in the reactor. Until now, polymer powders (PE, PP) for oxygen containing groups creation and montmorilonite powder (catalysis, biomediacal applications) were investigated.

**Keywords describing research area:**

Plasma treatment of powders

**Competence**

**Relevance for applied and industrial research:**

Suitable as testing plant for powder treatment.

**Relevance for fundamental studies:**

Investigation of new powder materials